For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

Remove the left side rear weatherstrip. Refer to Folding Top Side Rear Weatherstrip Replacement.

1 | Folding Top Left Side Rear Weatherstrip Retainer Screws (Qty: 4) Tighten 9 N·m (80 lb in)
2 | Folding Top Left Side Rear Weatherstrip Retainer Tip

• | Inspect the fit of the seal to door glass.

• | Cycle the top and inspect the joint between side front/rear rail weatherstrips.