For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement.
2. Disconnect the actuator electrical connectors from the air distribution case.

1 | Screw, Air Outlet Duct Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (14 lb in)
2 | Duct, Air Outlet
3 | Screw, Heater Core Cover Tighten 1.5 N·m (14 lb in)
4 | Cover, Heater Core
5 | Seal, Heater Core Pass Through
6 | Screw, Air Distribution Case Tighten 1.5 N·m (14 lb in)
7 | Case, Air Distribution
8 | Screw, Heater Core Bracket (Qty: 2) Tighten 1.5 N·m (14 lb in)
9 | Bracket, Heater Core
10 | Core, Heater