For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Folding Top Side Rear Weatherstrip Screw Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. The folding top must be partially open to remove the screw on the top edge of the weatherstrip.
2. Pull the weatherstrip out of the retainer.
3. Remove the rear weatherstrip retainer. Refer to Folding Top Side Rear Weatherstrip Retainer Replacement.

Tighten
3 N·m (26 lb in)

2 | Folding Top Rear Locating Pin/Locating Nut

#### Procedure

Reposition the rear weatherstrip to gain access to the rear locating pin/locating nut, remove the pin

Tighten
3 N·m (26 lb in)

3 | Folding Top Rear Weatherstrip Tip Ensure the folding top rear locating pin is in proper engagement position to the top and the body.