For 1990-2009 cars

### Removal Procedure

1. Remove the transmission fluid pan and filter. Refer to Automatic Transmission Fluid and Filter Replacement.
2. Disconnect the electrical wiring harness connector (3) from the output speed sensor (2).
3. Remove the output speed sensor bolt (3).
4. Remove the output speed sensor (2).
5. Remove the output speed sensor spacer (1).
6. Inspect the output speed sensor (2) for the following conditions:

• | Damaged or missing magnet

• | Damaged housing

• | Bent or missing electrical terminals

### Installation Procedure

1. Install the output speed sensor spacer (1).
2. Install the output speed sensor (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the output speed sensor bolt (3).

Tighten
Tighten the output speed sensor bolt to 11 N·m (97 lb in).

4. Connect the electrical wiring harness connector (3) to the output speed sensor (2).
5. Install the transmission fluid pan and filter. Refer to Automatic Transmission Fluid and Filter Replacement.