For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Fluid Irritant Caution in the Preface section. Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.
1 | Brake Pipe Fitting (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tip

• | Clean the area around the brake pipes and the proportioning valve of dirt and debris.

• | Note the location and routing of the brake pipes before removal.

• | Cap the brake pipe fittings to prevent fluid loss and contamination.

Tighten
20 N·m (15 lb ft)

2 | Proportioning Valve Bolt (Qty: 3) Tighten 10 N·m (89 lb in)
3 | Proportioning Valve Tip Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .