For 1990-2009 cars

Callout | Component Name
--- | ---

#### Procedure

1. Remove the headling rear trim panel. Refer to Headlining Rear Trim Panel Replacement
2. Remove the rear compartment lift window struts. Refer to Rear Compartment Lift Window Strut Replacement.

1 | Rear Compartment Lift Window Fastener (Qty :4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
Tighten the to Nuts 10 N·m (89 lb ).

2 | Rear Compartment Lift Window

#### Procedure

Check the rear compartment lift window for proper alignment before closing. Refer to Rear Compartment Lift Window Latch Replacement.