For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the upper radiator air baffle. Refer to Radiator Air Upper Baffle and Deflector Replacement .
3. Remove the fan shroud assembly. Refer to Cooling Fan and Shroud Replacement .
4. Remove the radiator inlet hose from the radiator. Refer to Radiator Inlet Hose Replacement .
5. Remove the radiator outlet hose from the radiator. Refer to Radiator Outlet Hose Replacement .
6. Remove the radiator support brackets. Refer to Radiator Support Bracket Replacement .

1 | A/C Condenser Bracket Bolt Tighten 9 N·m (80 lb in)
2 | A/C Condenser Bracket
3 | Radiator Assembly