For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Remove the I/P compartment. Refer to Instrument Panel Compartment Replacement.
2. Disconnect the blower motor resistor electrical connector.

1 | Screw, Blower Motor Resistor (Qty 2) Tighten 1.5 N·m (13 lb in)
2 | Resistor, Blower Motor