For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement .
2. Disconnect the fuel pump fuel feed line quick connect fitting (2) from the chassis line. Refer to Plastic Collar Quick Connect Fitting Service .
3. Remove the fuel pump fuel feed line.

### Installation Procedure

1. Install the fuel pump fuel feed line.
2. Connect the fuel pump fuel feed line quick connect fitting (2) to the chassis line. Refer to Plastic Collar Quick Connect Fitting Service .
3. Install the fuel tank. Refer to Fuel Tank Replacement .