For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the roof lift off panel window rear weatherstrip. Refer to Roof Lift Off Panel/Window Rear Weatherstrip Replacement

1 | Roof Lift Off Panel Window Rear Weatherstrip Retainer Fastener (Qty :8) Caution: Refer to Fastener Caution in the Preface section.

#### Preliminary Procedures

Remove the roof lift off panel window rear weatherstrip for just the side that is being repaired, Do Not remove the weatherstrip completely.

Tighten
Tighten the fastener to 2 N·m (89 lb in).

2 | Roof Lift Off Panel Window Rear Weatherstrip Retainer

#### Procedure

1. Clean the inside of the retainer and surface with a 50/50 mixture of isopropyl alcohol and water by volume on a dampened lint free cloth.
2. Peel the protective film from the foam tape on the back sides of the new retainer.
3. Insert the weatherstrip into the retainer starting in the center and working outwards and down the sides.