For 1990-2009 cars

## Instrument Cluster Trim Panel Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the shift control lever, if equipped with a manual transmission. Refer to Control Lever and/or Boot Replacement .
2. Remove the console shift lever bezel, if equipped with an automatic transmission. Refer to Console Shift Lever Bezel Replacement .
3. Remove the instrument panel (I/P) assist handle. Refer to Instrument Panel Assist Handle Replacement .

1 | I/P Cluster Trim Plate Assembly

#### Procedure

Disconnect the electrical connectors.

2 | Retainer Clip (Qty: 10)