For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Remove the Instrument Panel (I/P) carrier. Refer to Instrument Panel Carrier Replacement.

Note: Pull the tie bar far enough back for the air distribution duct to clear the opening.

2. Remove the I/P tie bar. Refer to Instrument Panel Tie Bar Replacement.

1 | Nut, Distributor Air Tighten 2.5 N·m (16 lb in)
2 | Bolt, Distributor Air Tighten 2.5 N·m (16 lb in)
3 | Distributor, Air