For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Nut | 10 N·m | 89 lb in
Air Cleaner Front Bolt/Nut | 10 N·m | 89 lb in
Air Cleaner Outlet Resonator Clamp | 9 N·m | 80 lb in
Brake Pipe | 20 N·m | 15 lb ft
Camshaft Position Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Purge Valve Bracket Bolt | 25 N·m | 18 lb ft
Fuel Fill Hose Clamp | 2.5 N·m | 22 lb in
Fuel Fill Pipe Ground Strap Bolt | 9 N·m | 80 lb in
Fuel Fill Pipe to Housing Bolt | 1.5 N·m | 13 lb in
Fuel Pump Module Access Cover Bolt | 10 N·m | 89 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Strap/Support Bolt | 22 N·m | 16 lb ft
Heated Oxygen Sensor (HO2S) | 41 N·m | 30 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor | 25 N·m | 18 lb ft
Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Screw | 0.6 N·m | 5 lb in
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in