For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor to Block Bolt | 22 N·m | 16 lb ft
Balance Shaft Adjustable Chain Guide Bolt | 10 N·m | 89 lb in
Balance Shaft Fixed Chain Guide Bolt | 12 N·m | 106 lb in
Balance Shaft Retaining Bolt | 10 N·m | 89 lb in
Block Coolant Plug | 15 N·m | 11 lb ft
Block Heater Bolt | 10 N·m | 89 lb in
Cam Cover to Cylinder Head Bolt | 10 N·m | 89 lb in
Cam Cover to Ground Cable Bolt | 10 N·m | 89 lb in
Cam Cover to Ground Cable Stud | 10 N·m | 89 lb in
Camshaft

- Camshaft Cap Bolt

10 N·m

89 lb in

- Camshaft Position Actuator Solenoid Valve Bolt

10 N·m

89 lb in

- Camshaft Position Sensor Bolt

10 N·m

89 lb in

- Camshaft Timing Chain Tensioner

75 N·m

55 lb ft

- Exhaust Camshaft Position Actuator -- Final Pass

30 N·m

22 lb ft

- Exhaust Camshaft Position Actuator -- First Pass

100 degrees

- Intake Camshaft Position Actuator -- First Pass

30 N·m

22 lb ft

- Intake Camshaft Position Actuator -- Final Pass

100 degrees

Catalytic Converter Bolt | 50 N·m | 37 lb ft
Catalytic Converter Bracket Bolt | 50 N·m | 37 lb ft
Catalytic Converter Nut | 50 N·m | 37 lb ft
Chain Guide Access Hole Plug | 90 N·m | 59 lb ft
Connecting Rod Bolt

- First Pass

25 N·m

18 lb ft

- Final Pass

100 degrees

Coolant Jacket Plug | 35 N·m | 26 lb ft
Crankshaft Balancer Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

125 degrees

Crankshaft Bearings - Lower Crankcase to Block - Bedplate

- First Pass

20 N·m

15 lb ft

- Final Pass

77 degrees

Crankshaft Position Reluctor Ring | 15 N·m | 11 lb ft
Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Cylinder Head Bolt

- First Pass

30 N·m

22 lb ft

- Final Pass

155 degrees

Cylinder Head Front Chain Case Bolt | 30 N·m | 22 lb ft
Cylinder Head Oil Gallery Plug | 35 N·m | 26 lb ft
Cylinder Head Opening Plate Bolt | 10 N·m | 89 lb in
Drive Belt Tensioner Bolt | 45 N·m | 33 lb ft
Engine Coolant Temperature Sensor | 20 N·m | 15 lb ft
Engine Lift Bracket Front Bolt | 25 N·m | 18 lb ft
Engine Lift Bracket Rear Bolt | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolt | 25 N·m | 18 lb ft
Exhaust Manifold to Turbocharger Stud | 10 N·m | 89 lb in
Exhaust Manifold to Cylinder Head Nut | 14 N·m | 10 lb ft
Exhaust Manifold to Cylinder Head Stud | 15 N·m | 11 lb ft
Flywheel Bolt - Automatic Transmission

- First Pass

53 N·m

39 lb ft

- Final Pass

25 degrees

Flywheel Bolt - Manual Transmission

- First Pass

53 N·m

39 lb ft

- Final Pass

25 degrees

Front Cover to Block Bolt | 25 N·m | 18 lb ft
Fuel Pipe Bracket Bolt | 10 N·m | 89 lb in
Fuel Pressure Dampener Bolt | 10 N·m | 89 lb in
Fuel Pressure Sensor | 33 N·m | 24 lb ft
Fuel Pump Bolt - High Pressure | 15 N·m | 11 lb ft
Fuel Pump - High Pressure Line | 30 N·m | 22 lb ft
Fuel Pump - Low Pressure Line | 30 N·m | 22 lb ft
Fuel Pump Cover | 10 N·m | 89 lb in
Fuel Rail Bolts | 22 N·m | 16 lb ft
Generator to Block Bolt | 22 N·m | 16 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Manifold Brace Bolt | 22 N·m | 16 lb ft
Intake Manifold to Cylinder Head Bolt | 22 N·m | 16 lb ft
Intake Manifold to Cylinder Head Nut | 22 N·m | 16 lb ft
Intake Manifold to Cylinder Head Stud | 15 N·m | 11 lb ft
Knock Sensor Bolt | 25 N·m | 18 lb ft
Lower Crankcase to Block Perimeter Bolt | 25 N·m | 18 lb ft
Oil Cooler Bolts | 22 N·m | 16 lb ft
Oil Filter Adapter Cover | 22 N·m | 16 lb ft
Oil Gallery Gerotor Cover - Rear Bolt | 6 N·m | 53 lb in
Oil Gallery Plug - Cylinder Head | 35 N·m | 26 lb ft
Oil Gallery Plug - Rear - Block | 60 N·m | 44 lb ft
Oil Level Indicator Tube Bolt | 10 N·m | 89 lb in
Oil Pan Baffle Bolt | 14 N·m | 10 lb ft
Oil Pan Bolts | 25 N·m | 18 lb ft
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pressure Switch | 26 N·m | 19 lb ft
Oil Pump Gerotor Cover Bolt | 6 N·m | 53 lb in
Oil Pump Pressure Relief Valve Plug | 40 N·m | 30 lb ft
Oxygen Sensor | 42 N·m | 31 lb ft
Piston Oil Squirter | 15 N·m | 11 lb ft
Power Steering Pump Bolt | 25 N·m | 18 lb ft
Power Steering Tensioner Bolt | 22 N·m | 16 lb ft
Spark Plug | 20 N·m | 15 lb ft
Starter Motor to Block Bolt | 53 N·m | 39 lb ft
Thermostat Housing to Block Bolts | 10 N·m | 89 lb in
Throttle Body Bolt | 10 N·m | 89 lb in
Throttle Body Nut | 10 N·m | 89 lb in
Timing Chain Adjustable Guide Bolt | 10 N·m | 89 lb in
Timing Chain Fixed Guide Bolt | 12 N·m | 106 lb in
Timing Chain Oil Nozzle Bolt | 10 N·m | 89 lb in
Timing Chain Tensioner Bolt | 10 N·m | 89 lb in
Timing Chain Upper Guide Bolt | 10 N·m | 89 lb in
Turbocharger Air Bypass Valve Cover Bolt/Screw | 7 N·m | 62 lb in
Turbocharger Air Cooler Outlet Pipe Bolts | 25 N·m | 18 lb ft
Turbocharger Brace Nut | 50 N·m | 37 lb ft
Turbocharger Coolant Feed Pipe Bolt | 20 N·m | 15 lb ft
Turbocharger Coolant Feed Pipe Mounting Bolt | 10 N·m | 89 lb in
Turbocharger Coolant Return Pipe Bolt | 20 N·m | 15 lb ft
Turbocharger Heat Shield Bolt | 10 N·m | 89 lb in
Turbocharger Nut | 30 N·m | 22 lb ft
Turbocharger Oil Feed Pipe Bolt | 20 N·m | 15 lb ft
Turbocharger Oil Return Pipe Bolt | 10 N·m | 89 lb in
Turbocharger Wastegate Regulator Solenoid Valve Bracket Bolt/Screw | 7 N·m | 62 lb in
Vacuum Pump Bolt | 10 N·m | 89 lb in
Vacuum Pump Bracket Bolt | 22 N·m | 16 lb ft
Vent Tube to Cylinder Head | 15 N·m | 11 lb ft
Water Jacket Drain Plug | 20 N·m | 15 lb ft
Water Pipe Support Bracket Bolt | 10 N·m | 89 lb in
Water Pump Access Cover Bolt | 10 N·m | 89 lb in
Water Pump/Balance Shaft Chain Tensioner Bolt | 10 N·m | 89 lb in
Water Pump Bolts | 25 N·m | 18 lb ft
Water Pump Drain Plug | 20 N·m | 15 lb ft
Water Pump Sprocket Bolt | 10 N·m | 89 lb in