For 1990-2009 cars

### Removal Procedure

1. Disconnect the mass air flow (MAF)/intake air temperature (IAT) sensor electrical connector (1).
2. Remove the MAF/IAT sensor screws.
3. Remove the MAF/IAT sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the MAF/IAT sensor.
2. Install the MAF/IAT sensor screws.

Tighten
Tighten the screws to 0.6 N·m (5 lb in).

3. Connect the MAF/IAT sensor electrical connector (1).