For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Caution: When performing service on or near the SIR components or the SIR wiring, the SIR system must be disabled. Refer to SIR Disabling and Enabling . Failure to observe the correct procedure could cause deployment of the SIR components, personal injury, or unnecessary SIR system repairs.
| Important: In order to prevent accidental deployment, the shorting bars close in order to short the connectors when the connectors are separated.