For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement .
2. Disconnect the blower motor resistor electrical connector.

1 | Blower Motor Resistor Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Blower Motor Resistor
3 | Blower Motor Screw (Qty: 3) Tighten 1.5 N·m (13 lb in)
4 | Blower Motor Assembly