For 1990-2009 cars

### Removal Procedure

1. Disconnect the intake camshaft position (CMP) sensor electrical connector.
2. Remove the CMP sensor bolt.
3. Remove the CMP sensor.

### Installation Procedure

Note: Inspect the CMP sensor for damage, replace as necessary.

1. Lubricate the CMP sensor O-ring seal with clean engine oil.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CMP sensor.
3. Install the CMP sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Connect the intake CMP sensor electrical connector.