For 1990-2009 cars

The following approximate capacities are given in English and metric conversions. See Fluid and Lubricant Recommendations for more information. All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

Application | Specification
--- | ---
Metric | English
Cooling System

- 2.0L - Automatic Transmission

8.7 liters

9.2 quarts

- 2.0L - Manual Transmission

9.0 liters

9.5 quarts

- 2.4L - Automatic Transmission

8.2 liters

8.7 quarts

- 2.4L - Manual Transmission

8.4 liters

8.9 quarts

Engine Oil With Filter

- 2.0L

4.8 liters

5.0 quarts

- 2.4L

4.8 liters

5.0 quarts

Fuel Tank | 51.5 liters | 13.6 gallons
Rear Differential Driveline/Axle - Locking/Limited Slip

- Drain and Fill With Cover Removed

1.2 liters

1.27 quarts

- Drain and Fill With Use of Drain Plug

1.1 liters

1.16 quarts

Rear Differential Driveline/Axle - Locking/Limited Slip Additive

- Limited Slip Additive Drain and Fill With Cover Removed

100 ml

3.38 oz

- Limited Slip Additive Drain and Fill With Use of Drain Plug

70 ml

2.37 oz

Transmission/Transaxle

- Automatic Transmission - 5L40-E/5L50-E - Bottom Pan Removal

7.0 liters

7.4 quarts

- Automatic Transmission - 5L40-E/5L50-E - Dry

8.5 liters

9.0 quarts

- Automatic Transmission - 5L40-E/5L50-E - Complete Overhaul

8.9 liters

9.4 quarts

- Manual Transmission - Aisin AR5

2.67 liters

2.75 quarts