For 1990-2009 cars

### Removal Procedure

1. Install the J 41623-B onto the transmission oil cooler (TOC) pipe.
2. Slide the J 41623-B toward the TOC pipe fitting.

Important: Rotate the J 41623-B to engage the TOC pipe fitting's retainer slots.

The J 41623-B should be nearly flush with the fitting.
3. Connect the J 41623-B onto the TOC pipe fitting.
4. Rotate the J 41623-B until the retainer clip (1) rises above the fitting retainer seat.
5. Pull back on the TOC pipe to disengage the pipe from the TOC pipe fitting.
6. Remove the J 41623-B from the TOC pipe.

### Installation Procedure

Important: Inspect the TOC pipe fitting and retaining clip for signs of wear or damage. Replace the components if necessary.

1. Install the TOC pipe into the TOC pipe fitting.

A distinct snap should be heard or felt when assembling the TOC pipe to the fitting.

2. To ensure the cooler line is properly installed, give the cooler pipe a gentle pull.