For 1990-2009 cars

#### Refrigerant System Capacities

Application | Specification
--- | ---
Metric | English
PAG Oil GM P/N 12378526 for United States PAG Oil GM P/N 88900060 for Canada
Abrupt Refrigerant Loss | 60 ml¹ | 2.0 oz¹
Compressor Replacement | 74 ml² | 2.5 oz²

- The Sanden PXV16 service compressor is used in this model year vehicle is precharged with 74 ml (2.5 oz) of PAG oil.

Condenser Replacement | 30 ml² | 1.0 oz²
Evaporator Replacement | 30 ml² | 1.0 oz²
Receiver Dehydrator Replacement | 30 ml² | 1.0 oz²

- Total System PAG Oil Capacity

118 ml

4.0 oz

R-134a

- Refrigerant Charge

0.47 kg

1.03 lbs

¹Abrupt refrigerant loss due to large leak, hose rupture, collision, or pressure relief valve opening. Conditions that allow the refrigerant to seep or bleed off over time do not cause this oil loss. Upon replacement of a component that caused a large refrigerant loss, also add the required amount of oil for the particular component.

²If more than the specified amount of PAG oil was drained from a component, add the equal amount of oil drained.