For 1990-2009 cars

## Radiator Inlet Hose Replacement LE5

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Resonator Replacement for the 2.4L engine.
3. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement for the 2.4L engine.

1 | Radiator Inlet Hose Assembly Tip Using SA9111E position radiator inlet hose clamps aside and remove hose from the fittings.

## Radiator Inlet Hose Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement for the 2.0L engine.
3. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement for the 2.0L engine.

1 | Radiator Inlet Hose Assembly Tip Using SA9111E position radiator inlet hose clamps aside and remove hose from the fittings.