For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement.
2. Remove the intake manifold cover studs.
3. Remove the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement.
4. Reposition the positive crankcase ventilation (PCV) hose clamp.
5. Remove the PCV hose from the cover.
6. Disconnect the intake (1) and exhaust (2) camshaft position actuator solenoid valve electrical connectors.
7. Remove the engine harness clip (1) from the cam cover.
8. Remove the engine harness bracket (1) from the intake manifold cover stud.
9. Disconnect the evaporative emission (EVAP) canister purge solenoid valve electrical connector (1).
10. Remove the engine harness clip (2) from the EVAP purge solenoid bracket.
11. Remove the engine harness clips (3, 4) from the cam cover.
12. Remove the ignition coils. Refer to Ignition Coil Replacement.
13. Remove the camshaft cover bolts.
14. Remove the camshaft cover.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the camshaft cover and bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

2. Install the ignition coils. Refer to Ignition Coil Replacement.
3. Install the engine harness clips (3, 4) to the cam cover.
4. Install the engine harness clip (2) to the EVAP purge solenoid bracket.
5. Connect the EVAP canister purge solenoid valve electrical connector (1).
6. Install the engine harness bracket (1) to the intake manifold cover stud.
7. Install the engine harness clip (1) to the cam cover.
8. Connect the intake (1) and exhaust (2) camshaft position actuator solenoid valve electrical connectors.
9. Install the PCV hose from the cover.
10. Position the PCV hose clamp.
11. Install the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement.
12. Install the intake manifold cover studs.

Tighten
Tighten the studs to 9 N·m (80 lb in).

13. Install the intake manifold cover. Refer to Intake Manifold Cover Replacement.