For 1990-2009 cars
Door Ajar Switch: The scan tool displays Door Closed or Door Ajar. This is the state of the door ajar switch as commanded by the BCM.
Door Ajar Switch: The scan tool displays voltage. This is the value of the voltage drop across the door ajar switch.
Door Lock Switch: The scan tool displays Lock, Unlock, or Idle. This is the state of the door lock switch as commanded by the BCM.
Door Lock Switch: The scan tool displays volts. This is the value of the voltage at the door lock switch signal circuit.
Driver Door Ajar Sw: The scan tool displays Door Closed or Door Ajar. This is the state of the driver door ajar switch as commanded by the BCM.
Driver Door Lock Actuator Command: The scan tool displays Lock, Unlock, Idle, or Invalid. This is the state of the driver door lock actuator switch as commanded by the BCM.
Fob 1 Programmed: The scan tool displays whether a keyless entry transmitter is currently programmed into the #1 slot.
Fob 1 Function: The scan tool indicates the last keyless entry function commanded by the keyless entry transmitter programmed to the #1 slot.
Fob 1 Battery: The scan tool displays the current battery state of the keyless entry transmitter battery as either Low or OK.
Fob 2 Programmed: The scan tool displays whether a keyless entry transmitter is currently programmed into the #2 slot.
Fob 2 Function: The scan tool indicates the last keyless entry function commanded by the keyless entry transmitter programmed to the #2 slot.
Fob 2 Battery: The scan tool displays the current battery state of the keyless entry transmitter battery as either Low or OK.
Fob 3 Programmed: The scan tool displays whether a keyless entry transmitter is currently programmed into the #3 slot.
Fob 3 Function: The scan tool indicates the last keyless entry function commanded by the keyless entry transmitter programmed to the #3 slot.
Fob 3 Battery: The scan tool displays the current battery state of the keyless entry transmitter battery as either Low or OK.
Fob 4 Programmed: The scan tool displays whether a keyless entry transmitter is currently programmed into the #4 slot.
Fob 4 Function: The scan tool indicates the last keyless entry function commanded by the keyless entry transmitter programmed to the #4 slot.
Fob 4 Battery: The scan tool displays the current battery state of the keyless entry transmitter battery as either Low or OK.
Last Fob Used: The scan tool indicates the last keyless entry transmitter that used the keyless entry system.
Passenger Door Lock Actuator Command: The scan tool displays Lock, Unlock, Idle, or Invalid. This is the state of the passenger door lock actuator switch as commanded by the BCM.
Trunk Ajar Switch: The scan tool displays Trunk Ajar or Trunk Closed. This is the state of the trunk ajar switch as monitored by the BCM. Active is displayed when the trunk is open. Inactive is displayed when the trunk is closed.
Trunk Motor: The scan tool displays Off/On. This is the state of the trunk motor as monitored by the BCM.
Trunk Release Solenoid Command: The scan tool displays Off or On. This is the state of the trunk release solenoid as commanded by the BCM.
Trunk Release Switch: The scan tool displays Inactive or Active. This is the state of the trunk release switch as commanded by the BCM.