For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Open the folding top and stowage compartment lid.
2. Remove the upper garnish molding. Refer to Windshield Upper Garnish Molding Replacement .

1 | Bolts, Striker Header (Qty: 3) Tighten 8 N·m (70 lb in)
2 | Striker, Header