For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.

1 | Lower Front Fascia Support Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Lower Front Fascia Support