For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery. Refer to Battery Negative Cable Disconnection and Connection.

1 | Underhood Electrical Center/Junction Block Cover Tab (Qty: 2)

#### Procedure

To remove the junction block cover use a flat-bladed tool to release the tab.

2 | Underhood Electrical Center/Junction Block Power Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tip The bolts are part of the underhood electrical center/junction block power. Tighten
10 N·m (89 lb in)

3 | Underhood Electrical Center/Junction Block Nut

#### Procedure

Disconnect the battery positive cable from the junction block by removing the nut.

Tighten
7 N·m (62 lb in)

4 | Underhood Electrical Center/Junction Block Tab (Qty: 6)

#### Procedure

Remove the electrical center/junction block by using a hook-like tool to disengage the tabs.

5 | Underhood Electrical Center or Junction Block Lower Cover Bolt

#### Procedure

Remove the electrical connector inside the block before removing the lower cover.

Tighten
20 N·m (15 lb ft)

6 | Underhood Electrical Center or Junction Block Lower Cover Nut

#### Procedure

Remove the electrical connector inside the block before removing the lower cover.

Tighten
7 N·m (62 lb ft)