For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the 3 wheelhouse liner screws, then remove the 3 push pins and pull rearward on the front liner.
3. Disconnect the fog lamp bulb socket electrical connector.

1 | Front Fog Lamp Assembly Screws (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Fog Lamp Assembly Tip Remove the lamp assembly from the fog lamp bracket.
3 | Front Fog Lamp Bulb Caution: Refer to Halogen Bulb Caution in the Preface section. Tip Turn the bulb socket counterclockwise and remove from the fog lamp assembly.
4 | Adjuster Screw

#### Procedure

Remove the screw in order to separate the fog lamp from the fog lamp ring.