For 1990-2009 cars

#### Special Tools

• | J 43653 Flywheel Holding Tool

• | J 45059 Angle Meter

#### Engine Flywheel with Manual Transmission

1. Install the clutch pilot bearing for manual transmission. Refer to Clutch Pilot Bearing Replacement.
2. Install the flywheel.
3. Install the NEW bolts.
4. Install J 43653 in the starter assembly location, engaging the flywheel, in order to prevent crankshaft rotation.

Notice: Refer to Fastener Notice in the Preface section.

5. Tighten the flywheel bolts.

Tighten
Tighten the flywheel bolts to 53 N·m (39 lb ft), plus 25 degrees, using the J 45059 .

#### Engine Flywheel with Automatic Transmission

1. Install the flywheel.
2. Install the NEW bolts.
3. Install J 43653 in the starter assembly location, engaging the flywheel, in order to prevent crankshaft rotation.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the flywheel bolts.

Tighten
Tighten the flywheel bolts to 53 N·m (39 lb ft), plus 25 degrees, using the J 45059 .