For 1990-2009 cars

### Removal Procedure

Note: The folding top will be required to be opened and supported.

1. Remove the left and right side front weatherstrips. Refer to Folding Top Side Front Weatherstrip Replacement.
2. Remove the left and right side front weatherstrip retainers. Refer to Folding Top Side Front Weatherstrip Retainer Replacement.
3. Open and support the folding top.
4. Remove the folding top cover number 1 bow retainer. Refer to Folding Top Cover Number 1 Bow Retainer Replacement.

Note: The folding top cover retainer flaps are glued to the front side rail and to the number 1 bow.

5. Fold back the front and side edge of the folding top cover by releasing the retainer strips to expose the latch, springs and cables.
6. Remove the folding top front latch if required. Refer to Folding Top Front Latch Replacement.
7. Disconnect the cables and springs from the number 1 bow. Refer to Folding Top Cover Rear Side Tension Cable Replacement or Folding Top Cover Front Side Tension Cable Replacement.
8. With the aid of an assistant, remove the screws (1) from the folding top number 1 bow panel rear mounting point.
9. With the aid of an assistant, remove the folding top number 1 bow panel (2) from midrear mounting point.

### Installation Procedure

1. With the aid of an assistant, loose fit folding top number 1 bow panel (2).
2. Position folding top number 1 bow panel for best fit.
3. Close and latch the top.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the screws (1) to the folding top number 1 bow panel midrear mounting point.

Tighten
Tighten the screws to 10 N·m (89 lb in).

5. Connect the cables and springs to the number 1 bow. Refer to Folding Top Cover Rear Side Tension Cable Replacement or Folding Top Cover Front Side Tension Cable Replacement.
6. Install the folding top front latch if required. Refer to Folding Top Front Latch Replacement.

Note: The old adhesive must be removed and follow the manufacture directions for the new adhesive.

7. Reposition the front and side edge of the folding top cover retainer strips and glue into position. Use 3M™ trim glue or equivalent.
8. Install the left and right side front weatherstrip retainers. Refer to Folding Top Side Front Weatherstrip Retainer Replacement.
9. Install the left and right side front weatherstrips. Refer to Folding Top Side Front Weatherstrip Replacement.
10. Install the folding top cover number 1 bow retainer. Refer to Folding Top Cover Number 1 Bow Retainer Replacement.
11. Inspect the folding top for proper fit and operation. Refer to Folding Top Adjustment.