For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air cleaner outlet resonator duct. Refer to Air Cleaner Outlet Resonator Replacement.
2. Disconnect the mass air flow (MAF)/intake air temperature (IAT) sensor electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

3. Remove the air cleaner front bolt or nut.

Tighten
10 N·m (89 lb in)

1 | Air Cleaner Assembly Tip Firmly tug on the air cleaner in order to disengage the air cleaner from the studs.