For 1990-2009 cars

## Folding Top Side Front Weatherstrip Replacement Prior to VIN 7Y103259

Callout | Component Name
--- | ---

#### Preliminary Procedures

Open and support the folding top.

1 | Folding Top Side Front Weatherstrip Screw Notice: Refer to Fastener Notice in the Preface section. Tip Prior to the listed VIN breakpoint, some vehicles may have been built with the second design weatherstrip. Tighten
10 N·m (89 lb in)

2 | Folding Top Side Front Weatherstrip Tip

1. Loosen both corners of the weatherstrip before pulling the weatherstrip away from the retainer.
2. Ensure both corners fit tight into the retainer ends when installing.

## Folding Top Side Front Weatherstrip Replacement After VIN 7Y103259

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open and support the folding top.

1 | Folding Top Side Front Weatherstrip Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Folding Top Side Front Weatherstrip Tip

• | Loosen both corners of the weatherstrip before pulling the weatherstrip away from the retainer.

• | Ensure both corners fit tight into the retainer ends when installing.