For 1990-2009 cars

## Windshield Wiper Motor Replacement Sky

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
3. Remove the wiper drive system module. Refer to Windshield Wiper Transmission Replacement.

1 | Windshield Wiper Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4.5 N·m (40 lb in)
2 | Windshield Wiper Motor Assembly

#### Procedure

1. Use the J 39232 , or equivalent, to separate the transmission arm from the wiper motor crank arm pivot.
2. Use the J 39529 , or equivalent, to install the transmission arm onto the wiper motor crank arm pivot.

#### Special Tools

• | J 39232 Wiper Linkage Separator

• | J 39529 Wiper Linkage Installer

## Windshield Wiper Motor Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
3. Remove the wiper drive system module. Refer to Windshield Wiper Transmission Replacement.

1 | Windshield Wiper Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4.5 N·m (40 lb in)
2 | Windshield Wiper Motor Assembly

#### Procedure

1. Use the J 39232 , or equivalent, to separate the transmission arm from the wiper motor crank arm pivot.
2. Use the J 39529 , or equivalent, to install the transmission arm onto the wiper motor crank arm pivot.

#### Special Tools

• | J 39232 Wiper Linkage Separator

• | J 39529 Wiper Linkage Installer