For 1990-2009 cars

Connector 1: | Body Control Module Label (Early Production)
Connector 2: | Body Control Module Label (Late Production)
Connector 3: | Body Control Module - Top View
Connector 4: | Body Control Module C1
Connector 5: | Body Control Module C2
Connector 6: | Body Control Module C3
Connector 7: | Body Control Module - Bottom View
Connector 8: | Body Control Module C4
Connector 9: | Fuse Block - Underhood Label (LE5 w/MA5)
Connector 10: | Fuse Block - Underhood Label (LE5 w/M82)
Connector 11: | Fuse Block - Underhood Label (LNF w/MA5)
Connector 12: | Fuse Block - Underhood Label (LNF w/M82)
Connector 13: | Fuse Block - Underhood Top View
Connector 14: | Fuse Block - Underhood Bottom View
Connector 15: | Fuse Block - Underhood C1
Connector 16: | Fuse Block - Underhood C2
Connector 17: | Fuse Block - Underhood C3
Connector 18: | Fuse Block - Underhood C4

### Body Control Module Label (Early Production)

### Body Control Module Label (Late Production)

#### Body Control Module - Label Usage

No. | Device | Rating | Description
--- | --- | --- | ---
1 | FUSE PLR | -- | --
2 | SPARE (Early Production) | -- | Spare Fuse
EMPTY (Late Production) | -- | Not Used
3 | SPARE (Early Production) | -- | Spare Fuse
EMPTY (Late Production) | -- | Not Used
4 | SPARE (Early Production) | -- | Spare Fuse
EMPTY (Late Production) | -- | Not Used
5 | SPARE (Early Production) | -- | Spare Fuse
EMPTY (Late Production) | -- | Not Used
6 | AMP Fuse | 20A | Audio Amplifier
7 | CLSTR Fuse | 10A | Instrument Panel Cluster
8 | IGN SW/PK3+ Fuse | 2A | Ignition Switch
9 | STOP LP Fuse | 10A | Not Used
10 | HVAC/PK3+ Fuse | 10A | Theft Deterrent Module and HVAC Control Module
11 | EMPTY | -- | Not Used
12 | SPARE Fuse | 20A | Spare Fuse
13 | AIRBAG Fuse | 10A | Inflatable Restraint Sensing and Diagnostic Module (SDM) and Inflatable Restraint Passenger Presence System (PPS) Module
14 | SPARE Fuse | 10A | Spare Fuse
15 | WPR Fuse | 10A | Windshield Wiper/Washer Switch
16 | HVAC/IP IGN Fuse | 10A | Clutch Start Switch (MA5), Fuse Block - Underhood (M82), HVAC Control Module, Inflatable Restraint Passenger Air Bag ON/OFF Indicator, and Instrument Panel Cluster (IPC)
17 | EMPTY | -- | Not Used
18 | EMPTY | -- | Not Used
19 | EPS/STR WHL CNTRL Fuse | 2A | Inflatable Restraint Steering Module Coil
20 | S ROOF Fuse (Early Production) | 15A | Not Used
SPARE (Late Production) | 15A | Spare Fuse
21 | SPARE Fuse | 20A | Spare Fuse
22 | EMPTY | -- | Not Used
23 | RDO Fuse | 15A | Radio
24 | SDM Fuse | 10A | Inflatable Restraint Sensing and Diagnostic Module (SDM)
25 | ECM/TCM Fuse | 10A | Engine Control Module (ECM) and Transmission Control Module (TCM) (M82)
26 | DR LCK Fuse | 15A | DOOR LOCK PCB Relay, DOOR UNLOCK PCB Relay, and DR DOOR UNLOCK PCB Relay
27 | INT LIGHT Fuse | 10A | INADVERTENT LOAD CONTROL PCB Relay
28 | EMPTY (Early Production) | -- | Not Used
SWC BKLT (Late Production) | 2A | Steering Wheel Control Switch - Left and Steering Wheel Control Switch - Right
29 | PWR WNDW Fuse | 30A | Window Switch - Driver and Window Switch - Passenger
30 | HVAC Relay | -- | Blower Motor and Blower Motor High Speed Relay
31 | EMPTY | -- | Not Used
32 | RAP Relay | -- | PWR WNDW and S ROOF Fuses
Printed Circuit Board (PCB) Relays - Not Serviceable
-- | DOOR LOCK PCB Relay | -- | Door Latch - Driver and Door Latch - Passenger
-- | DOOR UNLOCK PCB Relay | -- | Door Latch - Passenger
-- | DR DOOR UNLOCK PCB Relay | -- | Door Latch - Driver
-- | INADVERTENT LOAD CONTROL PCB Relay | -- | Inside Rearview Mirror

### Body Control Module - Top View

### Body Control Module C1

#### Connector Part Information

- OEM: 15393122
- Service: 88987847
- Description: 72-Way F Micro-64 Unsealed (GY)

#### Terminal Part Information

- Pins: 6-8, 13-17, 19, 22, 26, 31, 35, 40, 44, 47, 51, 53-57, 60-61
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

- Pins: 33, 38
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | WH | 682 | Door Lock/Unlock Signal
7 | WH | 682 | Door Lock/Unlock Signal
8 | WH | 1080 | Park Lamp Relay Control
9-12 | -- | -- | Not Used
13 | PK | 849 | Brake Fluid Level Sensor Signal
14 | L-BU | 1134 | Park Brake Switch Signal
15 | YE | 5199 | Run/Crank Relay Coil Control
16 | WH | 193 | Rear Defog Relay Control
17 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
18 | -- | -- | Not Used
19 | TN/WH (early) PK/WH (late) | 746 | Right Front Door Ajar Switch Signal
20-21 | -- | -- | Not Used
22 | GY/BK | 745 | Left Front Door Ajar Switch Signal
23-25 | -- | -- | Not Used
26 | L-GN | 1478 | Coolant Level Switch Signal
27-30 | -- | -- | Not Used
31 | L-BU | 20 | Stop Lamp Supply Voltage
32 | -- | -- | Not Used
33 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
34 | -- | -- | Not Used
35 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
36-39 | -- | -- | Not Used
40 | L-BU | 1788 | Traction Control Switch Signal
41-43 | -- | -- | Not Used
44 | TN/WH | 1969 | Headlamp High Beam Relay Control
45-46 | -- | -- | Not Used
47 | YE | 196 | Windshield Wiper Motor Park Switch Signal
48-50 | -- | -- | Not Used
51 | D-GN | 113 | Windshield Wiper Switch Signal 2
52 | -- | -- | Not Used
53 | L-BU | 20 | Stop Lamp Supply Voltage
54 | YE | 317 | Fog Lamp Relay Control
55 | OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
56 | OG/BK | 737 | Rear Compartment Lamp Control
57 | BN | 253 | Trunk Release Relay Control
58 | D-BU | 38 | Backup Lamp Relay Control (M82)
59 | -- | -- | Not Used
60 | TN | 28 | Horn Relay Control
61 | BK/WH | 651 | Ground
62-66 | -- | -- | Not Used
67 | YE | 61 | Outside Ambient Temperature Sensor Return
68-69 | -- | -- | Not Used
70 | D-GN/WH | 636 | Outside Ambient Temperature Sensor Signal
71 | L-GN/BK | 592 | DRL Relay Control
72 | -- | -- | Not Used

### Body Control Module C2

#### Connector Part Information

- OEM: 15393121
- Service: 88987848
- Description: 72-Way F Micro-64 Unsealed (GY)

#### Terminal Part Information

- Pins: 1-5, 9-11, 14-20, 26, 31, 33, 38, 44, 47, 51, 56-59, 61-62, 66-69, 71-72
- Terminal: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Body Control Module C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN/BK | 2500 | High Speed GMLAN Serial Data (+)
2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+)
3 | PK/WH | 1970 | Low Beam Headlamp Relay Output - Coil
4 | PU | 524 | Headlamp Dimmer Switch High Beam Signal
5 | BN/WH | 301 | Park Lamp Switch On Signal
6-8 | -- | -- | Not Used
9 | WH | 111 | Hazard Switch Signal
10 | TN | 1576 | Rear Compartment Lock Actuator Unlock
11 | D-GN | 264 | Security Indicator Control
12-13 | -- | -- | Not Used
14 | TN | 28 | Horn Relay Control
15 | WH | 103 | Headlamp Switch Headlamps On Signal
16 | OG | 192 | Front Fog Lamp Switch Signal
17 | PU/WH | 549 | Headlamp Switch Headlamps Off Signal
18 | WH | 5359 | 5-Volt Reference
19 | TN | 2501 | High Speed GMLAN Serial Data Bus (-)
20 | TN | 2501 | High Speed GMLAN Serial Data (-)
21-25 | -- | -- | Not Used
26 | D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal
27-30 | -- | -- | Not Used
31 | YE | 5361 | Brake Pedal Position Sensor Signal
32 | -- | -- | Not Used
33 | YE | 317 | Fog Lamp Relay Control
34-37 | -- | -- | Not Used
38 | L-GN/BK | 5060 | Low Speed GMLAN Serial Data
39-43 | -- | -- | Not Used
44 | L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
45-46 | -- | -- | Not Used
47 | YE/BK | 1138 | DRL Ambient Light Sensor Low Reference
48-50 | -- | -- | Not Used
51 | BN | 1356 | Flash To Pass Switch Signal
52-55 | -- | -- | Not Used
56 | WH | 1390 | Off/Run/Crank Voltage
57 | GY | 112 | Windshield Wiper Switch Signal 2
58 | PU | 719 | Low Reference
59 | BN | 5360 | Low Reference
60 | -- | -- | Not Used
61 | GY | 1884 | Cruise Control Switch Signal
62 | WH/BK | 1073 | 5-Volt Reference
63-65 | -- | -- | Not Used
66 | YE/BK | 1418 | Left Rear Turn Signal Switch Signal
67 | D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
68 | L-BU | 292 | Rear Defog Switch Signal
69 | D-GN/WH | 762 | A/C Request Signal
70 | -- | -- | Not Used
71 | PU | 5234 | Passenger Seat Belt Indicator
72 | WH | 193 | Rear Defog Relay Control

### Body Control Module C3

#### Connector Part Information

- OEM: 15492675
- Service: See Catalog
- Description: 41-Way F Metri-Pack 280 800 Series (RD)

#### Terminal Part Information

- Pins: A1, A3, A4, A5, A7, A8, A9, A10, A12, B1, D4, B3, B5, C12, D7
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins A1, A3, A4, A5, A7, A9, A10, A12, B1, B12, D4 - E/A
- Core/Insulation Crimp: Pins B3, B5, C12, D7 - E/C
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: C5, D1, D5, D6, D10, D12, D11
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: Pins C5, D1, D5, D6, D10, D12 - F/G
- Core/Insulation Crimp: Pins D11 - A/B
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Body Control Module C3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | TN | 294 | Door Lock Actuator Unlock Control (A31)
A2 | -- | -- | Not Used
A3 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
A4 | GY | 295 | Door Lock Actuator Lock Control (A31)
A5 | GY | 295 | Door Lock Actuator Lock Control (A31)
A6 | -- | -- | Not Used
A7 | BN | 9 | Park Lamp Supply Voltage
A8 | PK | 339 | Ignition 1 Voltage
A9 | YE | 18 | Left Rear Turn Lamps Supply Voltage
A10 | GY | 157 | Courtesy Lamp Control
A11 | -- | -- | Not Used
A12 | D-GN | 19 | Right Rear Turn Lamps Supply Voltage
B1 | TN | 694 | Driver Door Lock Actuator Unlock Control (A31)
B2 | -- | -- | Not Used
B3 | RD/WH | 1240 | Battery Positive Voltage
B4 | -- | -- | Not Used
B5 | BN | 4 | Accessory Voltage
B6-B7 | -- | -- | Not Available
B8-B11 | -- | -- | Not Used
B12 | GY | 8 | Instrument Panel Lamp Supply Voltage
C1-C2 | -- | -- | Not Available
C3-C4 | -- | -- | Not Used
C5 | D-GN | 801 | Retained Accesory Power Fuse Supply Voltage (A31)
C6-C7 | -- | -- | Not Available
C8-C11 | -- | -- | Not Used
C12 | OG | 228 | Windshield Washer Pump Control
D1 | RD/BK | 142 | Battery Positive Voltage
D2-D3 | -- | -- | Not Used
D4 | RD/WH | 840 | Battery Positive Voltage
D5 | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage (A31)
D6 | PK | 739 | Ignition 1 Voltage
D7 | PK | 1339 | Ignition 1 Voltage
D8-D9 | -- | -- | Not Used
D10 | RD/BK | 442 | Battery Positive Voltage
D11 | RD/WH | 640 | Battery Positive Voltage (UQ3)
D12 | RD/BK | 242 | Battery Positive Voltage

### Body Control Module - Bottom View

### Body Control Module C4

#### Connector Part Information

- OEM: 15492668
- Service: See Catalog
- Description: 68-Way F Metri-Pack 280 Series, Flexlock (L-GY)

#### Terminal Part Information

- Pins: F2, F4, F5, F6, F6
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: B1, C1, C8, C11, C12, D1, D3, E6, F1, F9, D10, D10
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins B1, C1, C8, C11, C12, D1, D3, E6, F1, F9 - E/C
- Core/Insulation Crimp: Pins D10- See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D4, E12
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: Pins D4 - F/G
- Core/Insulation Crimp: Pins E12 - A/B
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Body Control Module C4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A12 | -- | -- | Not Used
B1 | OG | 228 | Windshield Washer Pump Control
B2-B12 | -- | -- | Not Used
C1 | RD/WH | 1440 | Battery Positive Voltage
C2-C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8 | BN | 4 | Accessory Voltage
C9-C10 | -- | -- | Not Used
C11 | GY | 8 | Instrument Panel Lamp Supply Voltage
C12 | GY/BK | 1458 | Instrument Panel Lamp Feed - Secondary
D1 | RD/WH | 1040 | Battery Positive Voltage
D2 | -- | -- | Not Used
D3 | YE | 5199 | Run/Crank Relay Coil Control
D4 | BN | 141 | Ignition 3 Voltage
D5 | -- | -- | Not Used
D6-D7 | -- | -- | Not Available
D8-D9 | -- | -- | Not Used
D10 | RD/WH | 1140 | Battery Positive Voltage
D11-D12 | -- | -- | Not Used
E1-E5 | -- | -- | Not Used
E6 | PK | 439 | Ignition 1 Voltage
E7-E11 | -- | -- | Not Used
E12 | BK | 550 | Ground
F1 | RD/WH | 1540 | Battery Positive Voltage
F2 | GY | 8 | Instrument Panel Lamp Supply Voltage
F3 | -- | -- | Not Used
F4 | PK | 339 | Ignition 1 Voltage
F5 | PK | 339 | Ignition 1 Voltage
F6 | PK | 339 | Ignition 1 Voltage
F7-F8 | -- | -- | Not Used
F9 | PK | 1539 | Ignition 1 Voltage
F10-F12 | -- | -- | Not Used

### Fuse Block - Underhood Label (LE5 w/MA5)

### Fuse Block - Underhood Label (LE5 w/M82)

### Fuse Block - Underhood Label (LNF w/MA5)

### Fuse Block - Underhood Label (LNF w/M82)

#### Fuse Block - Underhood Usage

No. | Device | Rating | Description
--- | --- | --- | ---
1 | ENG COOL FAN Fuse (LNF) | 60A | Cooling Fan
2 | REAR DEFOG Fuse | 20A | Rear Window Defog Relay
3 | EMPTY | -- | Not Used
4 | BCM 3 Fuse | 30A | Body Control Module
5 | CRNK Fuse | 30A | Crank Relay
6 | BCM 2 Fuse | 40A | Body Control Module
7 | BCM Fuse | 50A | Body Control Module
8 | COOL FAN 2 Fuse (LE5) | 30A | Cooling Fan 2 Relay
9 | EMPTY | -- | Not Used
10 | TRUNK Fuse | 25A | Trunk Release Relay
11 | TRUNK Fuse | 5A | Trunk Release Relay
12 | EMPTY | -- | Not Used
13 | FUEL PUMP Fuse | 15A | Fuel Pump Relay
14 | REAR DEFOG Relay | -- | Defogger Grid
15 | A/C CLTCH Relay | -- | ECM, A/C Compressor Clutch
16-17 | EMPTY | -- | Not Used
18 | TRUNK RELSE Relay | -- | Trunk Lock Actuator, BCM
19 | FUEL PUMP Relay | -- | Fuel Pump and Sender Assembly
20 | EMPTY | -- | Not Used
21 | MIR Fuse | 5A | Power Mirror Switch
22 | A/C Fuse | 10A | A/C Clutch Relay
23 | EMPTY | -- | Not Used
24 | COOL FAN 2 Relay (LE5) | -- | Engine Cooling Fan, ECM
25 | FUSE PLR | -- | Not Used
26 | PWR/TRN | -- | EMISSIONS, INJ MOD, ECM Fuses
27 | EMPTY | -- | Not Used
28 | BCK/UP LAMP Relay (M82) | -- | BCK/UP LAMP Fuse
29 | DLC Fuse | 15A | Data Link Connector
30 | OUTLET Fuse | 20A | Cigar Lighter/Aux Power Outlet
31 | BCK/UP LAMP Fuse (M82) | 10A | Backup Lamp and Backup Lamp Switch (MA5)
32 | VAC PUMP Fuse (LNF) | 20A | VAC PUMP Relay (LNF)
33 | EMISSIONS Fuse | 10A | Heated Oxygen Sensor 1, 2, MAF Sensor, CPP Switch, EVAP Canister Purge Solenoid
34 | CRNK Relay | -- | Starter, ECM
35-36 | EMPTY | -- | Not Used
37 | PWR SEATS Fuse (AF2) | 20A | Seat Adjuster Switch - Driver
38 | VAC PUMP Relay (LNF) | -- | Brake Booster Pump Motor (LNF) and Engine Control Module (ECM)
39 | EMPTY | -- | Not Used
40 | COOL FAN 1 Fuse (LE5) | 30A | Cool Fan Relay
41 | TURBO Fuse (LNF) | 10A | Camshaft Position (CMP) Actuator Solenoid Exhaust, Camshaft Position (CMP) Actuator Solenoid Intake, Supercharger Boost Control Solenoid (LNF), and Turbo Bypass Valve Control Solenoid (LNF)
42 | ECM Fuse (LE5) | 15A | Engine Control Module
ECM Fuse (LNF) | 20A | Engine Control Module
43 | ECM/TRANS Fuse | 15A | ECM, TCM
44 | ABS Fuse (LE5) | 30A | Electronic Brake Control Module
ABS Fuse (LNF) | 40A | Electronic Brake Control Module
45 | INJ IGN MDL Fuse (LE5) | 10A | Fuel Injectors and Ignition Coils
INJ IGN MDL Fuse (LNF) | 15A | Ignition Coils
46 | BCK/UP LAMP Fuse (MA5) | 10A | Backup Lamps Switch
47 | EMPTY | -- | Not Used
48 | DRL Relay | -- | Body Control Module and Headlamp Low Beam - Left
49 | DRL Fuse | 15A | DRL Relay
50 | COOL FAN Relay (LE5) | -- | Cooling Fan
51 | RUN/CRNK Relay | -- | Starter
52 | WPR LO/HI Relay | -- | Wiper Motor
53 | FOG LAMP Fuse | 15A | FOG LAMP Relay
54 | FOG LAMP Relay | -- | Fog Lamp - LF and Fog Lamp - RF
55 | HORN Relay | -- | Horn Switch
56 | S BAND ONSTAR/RKE Fuse | 10A | Digital Radio Receiver (U2K), Remote Control Door Lock Receiver (RCDLR), and Vehicle Communication Interface Module (VCIM) (UE1)
57 | ABS Fuse | 10A | Electronic Brake Control Module
58 | DIODE WPR | -- | Wiper Relay
59 | WPR Fuse | 25A | Wiper Relay
60 | HORN Fuse | 10A | Horn Switch
61 | ABS Fuse | 20A | Electronic Brake Control Module
62 | I/P IGN Fuse | 20A | Body Control Module
63 | LT HI BEAM Fuse | 10A | Headlamp High Beam - Left
64 | CAN VENT Fuse | 10A | EVAP Canister Valve Solenoid
65 | LT LO BEAM Fuse | 10A | DRL Relay and Headlamp Low Beam - Left
66 | RT LO BEAM Fuse | 10A | Headlamp Low Beam - Right
67 | RT HI BEAM Fuse | 10A | Headlamp High Beam - Right
68 | PRK LAMPS Relay | -- | Body Control Module, License Lamp, Marker Lamp - LF, Marker Lamp - LR, Marker Lamp - RF, Marker Lamp - RR, Park Lamp - LF, Park Lamp - RF, Park/Turn Signal Lamp - LF, Park/Turn Signal Lamp - RF, Tail/Stop and Turn Signal Lamp - Left Outer, Tail/Stop and Turn Signal Lamp - Left Inner, Tail/Stop and Turn Signal Lamp - Right Inner, and Tail/Stop and Turn Signal Lamp - Right Outer
69 | PRK LAMPS Fuse | 15A | PRK LAMPS Relay
70 | WPR ON/OFF Relay | -- | Windshield Wiper Motor
71 | LO BEAM Relay | -- | LT LO BEAM Fuse, RT LO BEAM Fuse, and Body Control Module
72 | HI BEAM Relay | -- | LT HI BEAM Fuse, RT HI BEAM Fuse, and Body Control Module

### Fuse Block - Underhood Top View

### Fuse Block - Underhood Bottom View

### Fuse Block - Underhood C1

#### Connector Part Information

- OEM: R61927-002
- Service: 88988759
- Description: 64-Way F (GY)

#### Terminal Part Information

- Pins: E7
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

- Pins: A1, A9, A12, C9, D3, D9, D12, E6, E9, F1, F9, F10, F12
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: A10, A11, B10, B11, C4, C12
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fuse Block - Underhood C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | D-GN | 335 | Low Speed Cooling Fan Relay Control (LE5)
A2-A8 | -- | -- | Not Used
A9 | L-BU | 20 | Stop Lamp Supply Voltage
A10 | PK | 539 | Ignition 1 Voltage (MA5)
A11 | PK/BK | 5292 | Ignition 1 Voltage
A12 | BN | 4 | Accessory Voltage (M82)
B1 | -- | -- | Not Used
B2 | WH | 2368 | Cooling Fan Clutch Supply Voltage (LNF)
B3-B4 | -- | -- | Not Used
B5 | -- | -- | Not Available
B6-B7 | -- | -- | Not Used
B8 | -- | -- | Not Available
B9 | -- | -- | Not Used
B10 | PK/BK | 5290 | Ignition 1 Voltage
B11 | PK | 1039 | Ignition 1 Voltage (M82)
B12 | PK/BK | 5293 | Ignition 1 Voltage
C1-C3 | -- | -- | Not Used
C4 | L-GN | 24 | Backup Lamp Supply Voltage (MA5)
C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8 | -- | -- | Not Used
C9 | D-GN | 1433 | Clutch Start Switch Signal (LE5 w/MA5)
D-BU | 6306 | Clutch Start Switch Signal (LNF w/MA5)
C10-C11 | -- | -- | Not Used
C12 | PK | 1039 | Ignition 1 Voltage
D1-D2 | -- | -- | Not Used
D3 | BK | 250 | Ground
D4-D5 | -- | -- | Not Used
D6-D7 | -- | -- | Not Available
D8 | -- | -- | Not Used
D9 | PK/BK | 5291 | Ignition 1 Voltage
D10-D11 | -- | -- | Not Used
D12 | D-GN/WH | 459 | A/C Compressor Clutch Relay Control
E1-E4 | -- | -- | Not Used
E5 | -- | -- | Not Available
E6 | YE | 447 | Starter Relay Coil Control
E7 | PU | 6 | Starter Solenoid Crank Voltage
E8 | -- | -- | Not Available
E9 | PK/BK | 5291 | Ignition 1 Voltage
E10-E12 | -- | -- | Not Used
F1 | D-BU | 473 | High Speed Cooling Fan Relay Control (LE5)
F2 | L-GN | 24 | Backup Lamp Supply Voltage (LNF w/M82)
F3-F8 | -- | -- | Not Used
F9 | PK/BK | 5291 | Ignition 1 Voltage
F10 | D-GN | 59 | A/C Compressor Clutch Supply Voltage
F11 | -- | -- | Not Used
F12 | BN | 5069 | Main Relay Control (LE5)
YE | 5991 | Main Relay Control (LNF)

### Fuse Block - Underhood C2

#### Connector Part Information

- OEM: R61927-001
- Service: 88988756
- Description: 64-Way F (BK)

#### Terminal Part Information

- Pins: B6, B9
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: F6
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

- Pins: A1, B1, B3, B9, B10, B12, C1, D3, E1, E3, F1, F2
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: A5, F5
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: Pins A5 - D/G
- Core/Insulation Crimp: Pins F5 - A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: A9, E2, E12, F9, C2, E6, F3, F3
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: Pins A9, E2, E12, F9 - C/A
- Core/Insulation Crimp: Pins C2, E6, F3, F3 - E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fuse Block - Underhood C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
A2-A4 | -- | -- | Not Used
A5 | RD/BK | 142 | Battery Positive Voltage
A6-A8 | -- | -- | Not Used
A9 | RD/WH | 240 | Battery Positive Voltage
A10-A12 | -- | -- | Not Used
B1 | TN | 28 | Horn Relay Control
B2 | -- | -- | Not Used
B3 | RD/WH | 40 | Battery Positive Voltage
B4 | -- | -- | Not Used
B5 | -- | -- | Not Available
B6 | D-BU | 38 | Backup Lamp Relay Control (M82)
B7 | -- | -- | Not Used
B8 | -- | -- | Not Available
B9 | PK | 339 | Ignition 1 Voltage (M82)
YE | 575 | Starter Control (MA5)
B10 | PK/BK | 5291 | Engine Main Relay Fused Control
B11 | -- | -- | Not Used
B12 | WH | 193 | Rear Defog Relay Control
C1 | -- | -- | Not Used
C2 | L-GN | 24 | Backup Lamp Supply Voltage (M82)
C3-C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8-C12 | -- | -- | Not Used
D1-D2 | -- | -- | Not Used
D3 | RD/WH | 440 | Battery Positive Voltage
D4-D5 | -- | -- | Not Used
D6-D7 | -- | -- | Not Available
D8 | L-GN/BK | 592 | DRL Relay Control
D9-D12 | -- | -- | Not Used
E1 | TN/WH | 1969 | Headlamp High Beam Relay Control
E2 | GY | 120 | Fuel Pump Supply Voltage
E3 | BN | 253 | Trunk Release Relay Control
E4 | -- | -- | Not Used
E5 | -- | -- | Not Available
E6 | L-GN | 24 | Backup Lamp Supply Voltage (MA5)
E7 | -- | -- | Not Used
E8 | -- | -- | Not Available
E9-E11 | -- | -- | Not Used
E12 | PU | 293 | Rear Defog Element Supply Voltage
F1 | PK/WH | 1970 | Headlamp Low Beam Relay Control
F2 | D-GN/WH | 465 | Fuel Pump Primary Relay Control
F3 | TN/WH | 56 | Trunk Release Motor Supply Voltage
F4 | -- | -- | Not Used
F5 | RD/BK | 242 | Battery Positive Voltage
F6 | RD/BK | 442 | Battery Positive Voltage
F7-F8 | -- | -- | Not Used
F9 | BK | 250 | Ground
F10-F12 | -- | -- | Not Used

### Fuse Block - Underhood C3

#### Connector Part Information

- OEM: R61922-002-A
- Service: 88988760
- Description: 28-Way F (GY)

#### Terminal Part Information

- Pins: A5, E1
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

- Pins: A6, B1, B2, B5, C1, D6, E5, F1, F6
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: A3, F4
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: Pins A3 - D/G
- Core/Insulation Crimp: Pins F4 - A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: C5, E2
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: Pins C5 - C/A
- Core/Insulation Crimp: Pins E2 - E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fuse Block - Underhood C3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | RD/BK | 542 | Battery Positive Voltage
A4 | -- | -- | Not Used
A5 | RD/WH | 540 | Battery Positive Voltage
A6 | BN | 9 | Folding Top Stowage Compartment Lid
B1 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
B2 | TN/WH | 312 | Right Headlamp Low Beam Supply Voltage
B3-B4 | -- | -- | Not Available
B5 | YE | 712 | Left Headlamp Low Beam Supply Voltage
PU | 359 | DRL Supply Voltage
B6 | -- | -- | Not Used
C1 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
C2 | -- | -- | Not Used
C3-C4 | -- | -- | Not Available
C5 | BK | 250 | Ground
C6 | -- | -- | Not Used
D1-D2 | -- | -- | Not Used
D3-D4 | -- | -- | Not Available
D5 | PU | 359 | DRL Supply Voltage
D6 | PK | 1439 | Ignition 1 Voltage (JL9)
E1 | L-BU | 409 | Cooling Fan Motor Supply Voltage (LE5)
WH | 2368 | Cooling Fan Clutch Supply Voltage (LNF)
E2 | D-GN | 29 | Horn Control
E3-E4 | -- | -- | Not Available
E5 | PU | 2234 | Front Fog Lamp Supply Voltage
E6 | -- | -- | Not Used
F1 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
F2-F3 | -- | -- | Not Used
F4 | GY | 532 | Cooling Fan Motor Supply Voltage (LE5)
F5 | -- | -- | Not Used
F6 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage

### Fuse Block - Underhood C4

#### Connector Part Information

- OEM: R6-62807-001
- Service: 88988757
- Description: 28-Way F (BK)

#### Terminal Part Information

- Pins: C2
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

- Pins: F5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: D1, E1
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: A6, B2, B5, C1, C5, D6, D6, D6, E6, F2
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: A1, F3
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Fuse Block - Underhood C4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BN | 9 | Park Lamp Supply Voltage
A2-A5 | -- | -- | Not Used
A6 | L-BU | 20 | Stop Lamp Supply Voltage
B1 | -- | -- | Not Used
B2 | D-GN | 113 | Windshield Wiper Motor Relay Coil Supply Voltage
B3-B4 | -- | -- | Not Available
B5 | WH | 1080 | Park Lamp Relay Control
B6 | -- | -- | Not Used
C1 | L-GN | 1715 | Windshield Wiper Switch High Signal
C2 | PK | 739 | Ignition 1 Voltage
C3-C4 | -- | -- | Not Available
C5 | RD/WH | 140 | Battery Positive Voltage
C6 | -- | -- | Not Used
D1 | D-GN | 95 | Windshield Washer Switch Signal
D2 | -- | -- | Not Used
D3-D4 | -- | -- | Not Available
D5 | -- | -- | Not Used
D6 | RD/WH | 1340 | Battery Positive Voltage
E1 | PU | 92 | Windshield Wiper Motor High Speed Control
E2 | -- | -- | Not Used
E3-E4 | -- | -- | Not Available
E5 | -- | -- | Not Used
E6 | RD/WH | 1340 | Battery Positive Voltage
F1 | -- | -- | Not Used
F2 | YE | 5199 | Run/Crank Relay Coil Control
F3 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
F4 | -- | -- | Not Used
F5 | BN | 4 | Accessory Voltage (M82)
F6 | -- | -- | Not Used