For 1990-2009 cars

## Instrument Panel Trim Pad Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the instrument panel cluster (IPC) trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the driver knee bolster trim panel. Refer to Knee Bolster Replacement .
3. Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement .
4. Remove the I/P inflatable restraint. Refer to Inflatable Restraint Instrument Panel Module Replacement .
5. Remove the right and left I/P outer trim covers. Refer to Instrument Panel Outer Trim Cover Replacement - Right Side and Instrument Panel Outer Trim Cover Replacement - Left Side .
6. Remove the right and left windshield pillar garnish moldings. Refer to Windshield Pillar Garnish Molding Replacement .
7. Remove the I/P extension trim plate. Refer to Instrument Panel Extension Trim Plate Replacement .

1 | I/P Trim Pad Screw (Qty: 17) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | I/P Trim Pad Assembly

#### Procedure

Disconnect the electrical connectors.