For 1990-2009 cars

# Water Leak Down A-Pillar or Drips from Roof Header onto Shifter (Apply Sealer to Convertible Top Seam)

Subject: | Water Leak Down "A" Pillar or Drips from Roof Header onto Shifter (Apply Sealer to Convertible Top Seam)

Models: | 2006-2009 Pontiac Solstice

| 2007-2009 Saturn SKY

| 2007-2009 Opel GT

This bulletin is being revised to update the models and model years. Please discard Corporate Bulletin Number 06-08-67-016 (Section 08 - Body and Accessories).

### Condition

Some customers may comment on a water leak down the "A" pillar where the front top weatherstrip meets the windshield weatherstrip, or drips from the roof header onto the shifter.

### Cause

This condition may be caused by the transition at the convertible top seams being too big for the seal to overcome.

### Correction

Apply clear silicone sealer to the opening at the seam to smooth out the transition between the convertible top sections.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C9774* | Apply Sealer to Convertible Top Seam | 0.2 hr
*This is a unique labor operation for bulletin use only. It will not be published in the Labor Time Guide.