For 1990-2009 cars

## Front Side Door Window Regulator Replacement Manual

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Remove the front side door window. Refer to Front Side Door Window Replacement.

1 | Plug, Window Regulator Nut Access Tip Use a plastic flat-bladed tool to remove the plug from the bottom of the door.
2 | Nut, Front Side Door Window Regulator (Qty: 4) Tighten 10 N·m (89 lb in)
3 | Bolt, Front Door Window Regulator (Qty: 3) Tighten 10 N·m (89 lb in)
4 | Regulator, Front Door Manual Window

## Front Side Door Window Regulator Replacement Power

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Remove the front side door window. Refer to Front Side Door Window Replacement.

1 | Plug, Window Regulator Nut Access Tip Use a plastic flat-bladed tool to remove the plug from the bottom of the door.
2 | Nut, Front Side Door Window Regulator (Qty: 4) Tighten 10 N·m (89 lb in)
3 | Bolt, Front Door Window Regulator (Qty: 3) Tighten 10 N·m (89 lb in)
4 | Regulator, Front Door Power Window Tip Disconnect the electrical connector from the regulator.