For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Recover the A/C system. Refer to Refrigerant Recovery and Recharging .

1 | A/C Compressor Tube Assembly -- Nut Tighten 16 N·m (12 lb ft)
2 | Sealing Washer Tip Remove and discard the sealing washer. Refer to Sealing Washer Replacement .
3 | Thermal Expansion Valve Bolt Tighten 16 N·m (12 lb ft)
4 | Sealing Washer Tip Remove and discard the sealing washer. Refer to Sealing Washer Replacement .
5 | Thermal Expansion Valve