For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Folding Top Clock Spring Shaft Nut | 11 N·m | 97 lb in
Folding Top Cover Number 1 Bow Retainer Screws | 2 N·m | 18 lb in
Folding Top Cover Number 1 Bow Screws | 10 N·m | 89 lb in
Folding Top Cover Number 3 Bow Screws | 10 N·m | 89 lb in
Folding Top Cover Number 4 Bow Screws | 10 N·m | 89 lb in
Folding Top Cover Rear Retainer Nut/Bolt | 9 N·m | 80 lb in
Folding Top Front Latch Handle Nut | 21 N·m | 16 lb ft
Folding Top Front Latch Screws | 9 N·m | 80 lb in
Folding Top Front Latch Striker Header Bolt | 8 N·m | 70 lb in
Folding Top Front Locating Pin | 18 N·m | 13 lb ft
Folding Top Front Locating Pin Guide Bolt | 25 N·m | 18 lb ft
Folding Top Link Nut | 25 N·m | 18 lb ft
Folding Top Pivot Bracket Nut | 9 N·m | 80 lb in
Folding Top Rear Latch Bolts | 25 N·m | 19 lb ft
Folding Top Rear Latch Bracket Bolts | 25 N·m | 19 lb ft
Folding Top Rear Latch Striker Bolt | 11 N·m | 97 lb in
Folding Top Rear Latch Striker Screw | 2 N·m | 18 lb in
Folding Top Rear Locating Pin/Locating Nut | 3 N·m | 26 lb in
Folding Top Rear Side Rail Ball Stud | 12 N·m | 106 lb in
Folding Top Rear Side Rail Cable Roller Screw | 3 N·m | 26 lb in
Folding Top Rear Side Rail Screw | 20 N·m | 15 lb ft
Folding Top Side Rail Assembly Bolts | 10 N·m | 89 lb in
Folding Top Side Frame Assembly Fasteners | 9 N·m | 80 lb in
Folding Top Side Front Weatherstrip Screw - After VIN 67Y118652 | 2 N·m | 18 lb in
Folding Top Side Front Weatherstrip Screw - Prior to VIN 67Y118652 | 10 N·m | 89 lb in
Folding Top Side Front Weatherstrip Retainer Screws | 9 N·m | 80 lb in
Folding Top Side Rail Link Bolt | 9 N·m | 80 lb in
Folding Top Side Rail to Number 1 Bow Screws | 10 N·m | 89 lb in
Folding Top Side Rail to Number 3 Bow Screws | 10 N·m | 89 lb in
Folding Top Side Rail to Number 4 Bow Screws | 10 N·m | 89 lb in
Folding Top Side Rear Weatherstrip Screw - After VIN 67Y118652 | 3 N·m | 26 lb in
Folding Top Side Rear Weatherstrip Screw - Prior to VIN 67Y118652 | 10 N·m | 89 lb in
Folding Top Side Rear Weatherstrip Retainer Screws | 9 N·m | 80 lb in
Folding Top Stow Strap to Inner Quarter Panel Fasteners | 9 N·m | 80 lb in
Upstop Jam Nut | 17 N·m | 13 lb ft