For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel left closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Disconnect the clutch pedal position sensor electrical connector.

1 | Clutch Pedal Position Sensor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Clutch Pedal Position Sensor Warning: Replacement or reprogramming of the ECM, or replacement of the clutch pedal position sensor (CPPS) or clutch pedal requires that a CPPS learn procedure be performed. Failure to perform the CPPS learn procedure may result in personal injury or damage to the vehicle or its components if the vehicle is in gear and the starter motor is accidentally engaged.

#### Procedure

Perform the clutch pedal position sensor learn procedure. Refer to Clutch Pedal Position Sensor Learn.