For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Power Steering Fluid Cooling Pipe Bracket Bolts | 9 N·m | 80 lb in
Power Steering Fluid Reservoir Bolt | 9 N·m | 80 lb in
Power Steering Gear Inlet Hose Fitting | 27 N·m | 20 lb ft
Power Steering Gear Outlet Hose Bracket Bolts | 9 N·m | 80 lb in
Power Steering Gear Outlet Hose Fitting | 27 N·m | 20 lb ft
Power Steering Pump Belt Tensioner Bolt | 22 N·m | 16 lb ft
Power Steering Pump Bolts | 22 N·m | 16 lb ft
Power Steering Pump Bracket Bolts | 58 N·m | 43 lb ft
Steering Gear Bolts | 60 N·m | 44 lb ft
Steering Gear Nuts | 60 N·m | 44 lb ft
Steering Linkage Inner Tie Rod | 80 N·m | 60 lb ft
Steering Linkage Outer Tie Rod Nut | 30 N·m + 115 degrees | 22 lb ft +115 degrees