For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamps. Refer to Headlamp Replacement .

1 | Hood Hinge Nuts (Qty: 4) Tip

1. Disconnect the wiring harness from the hood on both sides.
2. Mark the hood for proper alignment for re-installing.

Notice: Refer to Fastener Notice in the Preface section.

Tighten
25 N·m (19 lb ft)

2 | Hood Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.