For 1990-2009 cars

## Control Lever and/or Boot Replacement Sky

Callout | Component Name
--- | ---
1 | Shift Boot Bezel Tip Grasp the edge of the shift boot bezel by reaching under the bezel from the soft boot area. Lift the shift boot bezel up to release the bezel from the instrument panel cluster trim plate.
2 | Shift Control Lever Retaining Screw Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Lift the shift boot up for access.
2. It is not necessary to fully remove the screw in order to release the control lever.
3. Ensure the screw is lined up with the flat on the transmission shift lever before tightening.

Tighten
10 N·m (89 lb in)

3 | Shift Control Lever Knob and Boot Tip The shift control lever knob and boot must be replaced as an assembly.

## Control Lever and/or Boot Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lift up the lower edge of the instrument panel cluster trim plate only enough to reach fingers underneath in order to release the shift boot bezel retaining tabs.

1 | Shift Control Lever Boot Bezel Tip Release the shift control boot bezel retaining tabs from the instrument cluster trim panel.
2 | Shift Control Lever Screw Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Lift the shift boot up for access.
2. It is not necessary to fully remove the screw in order to release the control lever.
3. Ensure the screw is lined up with the flat on the transmission shift lever before tightening.

Tighten
10 N·m (89 lb in)

3 | Shift Control Lever Knob Tip The shift control knob and boot must be replaced as an assembly.