For 1990-2009 cars

## Hood Ornament Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Reposition the hood insulator pad as required to access the hood ornament. Refer to Hood Insulator Replacement .
2. Remove the push nuts securing the hood ornament to the inside hood panel.
3. Using a J 25070 , warm the exterior hood ornament to a minimum of 21°C (70°F) to assist with the hood ornament adhesive tape removal and installation.

#### Special Tools

J 25070 Heat Gun

1 | Push Nut (Qty: 4)
2 | Adhesive Tape Tip When removing the protective liners from the adhesive tape, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3 | Hood Ornament Tip Secure the hood ornament with new push nuts in order to secure.