For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Replace the passenger presence system as a complete assembly to prevent possible injury to the occupant. All the components in the service kit are assembled and calibrated as a unit. Using only some of the components in the service kit will cause the passenger presence system to operate improperly.

#### Preliminary Procedure

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References .

1 | Nut, Seat Back Recliner Notice: Refer to Fastener Notice in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Retainer, Seat Cushion Cover (Qty: 4) Tip Use a J 38778 Door Trim Pad Clip Remover to aid in the removal of the seat cushion cover retainers.
3 | Cover, Seat Cushion Tip

1. Tilt the seat back forward.
2. Disconnect the seat cushion cover J-channel from the front and rear of the seat cushion frame.
3. Disconnect the electrical connector if working on the passenger seat.

4 | Pad, Seat Cushion Tip The passenger presence system is part of the pad on the passenger seat cushion, and must be replaced as an assembly.