For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Secure the steering wheel utilizing a strap to prevent rotation. Locking of the steering column will prevent damage and a possible malfunction of the SIR system. The steering wheel must be secured in position before disconnecting the following components:

• | The steering column

• | The intermediate shaft

• | The steering gear

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.

#### Preliminary Procedure

Remove the front tire/wheel assemblies. Refer to Tire and Wheel Removal and Installation

1 | Steering Linkage Outer Tie Rod Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 30 N·m (22 lb ft) plus an additional 115 degrees
2 | Steering Linkage Outer Tie Rod End (Qty: 2)

#### Procedure

Refer to Steering Linkage Outer Tie Rod Replacement for removal.

3 | Steering Gear Inlet and Outlet Hose Fitting (Qty: 2)

#### Procedure

Place drain pans under the vehicle as needed to catch any power steering fluid.

Tighten
27 N·m (20 lb ft)

4 | Steering Gear Bolt (Qty: 2) Tighten 60 N·m (44 lb ft)
5 | Steering Gear

#### Procedure

1. Remove the intermediate steering shaft lower bolt from the steering gear. Refer to Intermediate Steering Shaft Replacement.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.
3. Adjust the front toe. Refer to Front Toe Adjustment.