For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement .
2. Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement .
3. Remove the passenger side door sill plate. Refer to Door Sill Plate Replacement .
4. Remove the instrument panel (I/P) trim pad. Refer to Instrument Panel Trim Pad Replacement .

1 | Radio Antenna Cable Assembly

#### Procedure

The AM/FM radio antenna cable is part of the body electrical harness, to replace do the following :

1. Route the cable next to the body wiring harness and secure to the harness with tie straps.
2. Cut both ends of the original antenna cable.