For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement .
2. Disconnect the evaporative emission (EVAP) canister vent solenoid valve tube quick connect fitting. Refer to Plastic Collar Quick Connect Fitting Service .
3. Depress the locking tab on the EVAP canister vent solenoid valve mount and slide the valve out of the canister.

### Installation Procedure

1. Install the EVAP canister vent solenoid valve onto the mount on the canister, push the valve forward until the locking tab engages.
2. Connect the EVAP canister vent tube quick connect fitting. Refer to Plastic Collar Quick Connect Fitting Service .
3. Install the fuel tank. Refer to Fuel Tank Replacement .