For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement.
2. Remove the oil level indicator.
3. If the vehicle is equipped with a engine oil cooler, remove the radiator surge tank outlet hose clip from the oil level indicator tube.
4. Remove the engine harness clip (1) from the oil level indicator tube.
5. Remove the fuel line clip from the oil level indicator tube.
6. Remove the knock sensor clip from the oil level indicator tube.
7. Remove the oil level indicator tube bolt.
8. Remove the oil level indicator tube.

### Installation Procedure

1. Lubricate the oil level indicator tube O-ring seal with lubricant. Refer to Adhesives, Fluids, Lubricants, and Sealers for the correct part number.
2. Install the oil level indicator tube.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil level indicator tube bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the knock sensor clip to the oil level indicator tube.
5. Install the fuel line clip to the oil level indicator tube.
6. Install the engine harness clip (1) to the oil level indicator tube.
7. If the vehicle is equipped with a engine oil cooler, install the radiator surge tank outlet hose clip to the oil level indicator tube.
8. Install the oil level indicator.
9. Install the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement.