For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Open and support the folding top.

1 | Folding Top Side Front Weatherstrip Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Folding Top Side Front Weatherstrip Tip

• | Loosen both corners of the weatherstrip before pulling the weatherstrip away from the retainer.

• | Ensure that both corners fit tight into the retainer ends when installing.